Checklist of E/OHS Activities for Bleacher safety

Program Contact Person: 	Troy Stresemann					  

Is the BSM Plan in place? Yes No N/A 

Is the Plan current? Yes No N/A 

Has the Plan been reviewed this school year? Yes No N/A 

Has an annual survey of school bleachers been conducted? Yes No N/A 

Is the five-year recertification required by December 31, 2013 complete and submitted to the Minnesota Department of Labor and Industry? Yes No N/A

[bookmark: _GoBack]Note: The bleachers were surveyed 2/4/2013 by Brian Parrie. The paper work was submitted 2/5/2013.

Openings and gaps:

     X		Openings limited to four-inch gap between the railings and between the footboards and seat boards, starting at a height of 56 inches or more.

Retractable bleachers:

   X		They may contain openings of 9 inches or less

    N/A		If exempt from standards must have a safety management plan in place and an amortization schedule to plan for their future replacement

Approved netting:

   N/A		Netting may be provided to prevent persons from falling through the bleachers between the seat and footboards

   N/A		Chain link fencing may be used but must be secured tightly to the underside of the bleachers.

Railings:

    X		Bleachers 55 inches and under are exempt from railing requirements 

    X		Bleachers with guardrails over 30 inches above grade must not contain openings greater than four inches, unless safety nets are installed. 
    N/A		State building inspectors shall determine whether the safety nets and guardrail climb ability meet the requirements of the alternate design section of the State Building Code.


Periodic inspections:

     X		Bleacher footboards and guardrails must at a minimum be reinspected at least every five years and a structural inspection at least every ten years. The equipment has no rust, rot, cracks, or splinters, especially where it comes in contact with the ground



