**Client:** ECHO Charter

**Machine Name:** Freezer Compressor

**Location of Machine:** Kitchen

**Energy Type:** Electrical/Pneumatic

**Building:** School

**Client Contact:** Jim Stetteldahl

**Shutdown:**

**Step 1: Alert all employees that will be affected by the shut down.**

**Step 2: Shut machine down using normal shut down procedures.**

*Location & Method:*

* Turn the “thermostat” switch located on the unit to the “OFF” position

**Step 3: Isolate machine from all energy sources.**

*Location & Method:*

* Turn the “Rocker” arm that is located on the west wall of the boiler room to the “off” position

**Step 4: Apply Lockout devices.**

*Location:*

* Apply lockout device to electricity and whatever machine you are working on.
* Panel box -breakers 14,16,18

**Step 5: Verification & Dissipation of stored energy.**

*Location & Method:*

* Attempt to start by using the “On/Off” switch located on the unit.
* This unit is serviced by a refrigeration specialist only

**Shutdown:**

**MACHINE IS NOW LOCKED OUT**

**Start up**

**Step 1: Alert all employees of the start up**

**Step 2: Remove all Lockout devices.**

**Step 3: Restore energy to equipment.**

**Step 4: Verify restoration by starting equipment**