


Checklist of E/OHS Activities for Respiratory Protection

Program Contact Person: 	Brian Mohr					

Does this school provide respirators for voluntary use? Yes No N/A
If the school allows employees to use respirators voluntarily the following is mandatory.
1. Read and follow instructions provided by manufacturer.
2. Choose respirators certified for use against contaminants of concern.
3. Do not wear respirators in atmospheres containing contaminants not designed to protect from those contaminants.
4. Keep track of respirators so that you do not mistakenly wear someone else’s respirator.

Is the Respiratory Protection program in place?  Yes No N/A

Is the Plan current?  Yes No N/A

Has the Plan been reviewed this school year?  Yes No N/A

	Date of review: 	2011				


Are all employees in this program identified?  Yes No N/A

	
Employee
	
Intended Use
	
Type of Respirator
	
Medical Exam/
Questionnaire
	
Date of Medical
	
Date of
Fit Test

	
All voluntary use only
	Particulate matter
	NP95
	N/A
	N/A
	N/A

	

	
	
	
	
	

	

	
	
	
	
	

	

	
	
	
	
	

	

	
	
	
	
	

	

	
	
	
	
	









Fit testing was completed on       N/A.
		(date)

Type of testing protocol; Irritant Smoke (Stannic Chloride) or  
Bitrex (Denatonium Benzoate)



Condition and location of respirators:

	Condition: The condition is good


	Location(s): Only dust masks are used, they are in a like new condition.


Are the appropriate adequate accessories on hand?  Yes No N/A

Verified by:  Brian Parrie 3/2/2011






























APPENDIX D TO 1910.134 
INFORMATION FOR EMPLOYEES USING RESPIRATORS WHEN NOT REQUIRED UNDER THE STANDARD – MANDATORY

Respirators are an effective method of protection against designated hazards when properly selected and worn.  Respirator use is encouraged, even when exposures are below the exposure limit, to provide an additional level of comfort and protection for workers.  However, if a respirator is used improperly or not kept clean, the respirator itself can become a hazard to the worker.  Sometimes, workers may wear respirators to avoid exposures to hazards, even if the amount of hazardous substance does not exceed the limits set by OSHA standards.  If your employer provides respirators for your voluntary use, or if you provide your own respirator, you need to take certain precautions to be sure that the respirator itself does not present a hazard.


	You should do the following:

1. Read and heed all instructions provided by the manufacturer on use, maintenance, cleaning and care, and warnings regarding the respirator limitations.

2. Choose respirators certified for use to protect against the contaminant of concern.  NIOSH, the National Institute for Occupational Safety and Health of the U.S. Department of Health and Human Services, certifies respirators.  A label or statement of certification should appear on the respirator or respirator packaging.  It will tell you what the respirator is designed for and how much it will protect you.

3. Do not wear your respirator into atmospheres containing contaminants for which your respirator is not designed to protect against.  For example, a respirator designed to filter dust particles will not protect you against gases, vapors, or very small solid particles of fumes or smoke.

4. Keep track of your respirator so that you do not mistakenly use someone else’s respirator.


[63 FR 1270, Jan. 8, 1998;  63 FR 20098, Apr. 23, 1998]


Signature:_______________________________________________________________
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