Checklist of E/OHS Activities for Hearing Conservation

Program Contact Person: Barry Gappa

Is the Hearing Conservation Plan in place? *Yes No*

Is the Plan current? *Yes No*

Has the Plan been reviewed this school year? *Yes No*

Has the school been surveyed for noise hazards? *Yes No*

Have sound level measurements been collected? *Yes No*

Have the results been documented? *Yes No*

Location: Activities Manual

Has training been scheduled or completed for affected individuals this school year?

*Yes No N/A*

Date: 11/5/2014

Presenter: Brian Parrie

Have regulatory changes occurred that may affect this program? No

**Client:** Nicollet Public Schools

|  |  |  |  |
| --- | --- | --- | --- |
| **Measuring Device: Center 325 Sound Level Meter** | | **Calibration:**  Pre\_\_\_\_\_\_\_\_\_\_\_ Post\_\_\_\_\_\_\_\_\_\_\_ | |
| **Reason for Testing: General Survey** | | | |
| **Affected Personnel: Band Custodial, Maintenance, Shop** | | | |
| **Location** | **Equipment** | **Results** | **Recommendations** |
| Boiler room | boiler | 81.7 dBA |  |
| Shop | JD X485 | 77.dBA |  |
| Shop | JD 1435 | 73.9 dBA |  |
| Shop | Rockwell Drill Press | 81.5 dBA |  |
| Shop | Surface Planner | 91.87 dBA | Provide Protection |
| Shop | Makita Chop Saw | 91.9 dBA | Provide Protection |
| Shop | Porter Cable Router | 91.5 dBA | Provide Protection |
| Shop | Wood Lath | 80.0 dBA |  |
| Shop | Drum Sander | 87.0 dBA | Provide Protection |
| Shop | Powermatic Drill Press | 91.5 dBA | Provide Protection |
| Shop | Stationary belt sander | 81.5 dBA |  |
| Shop | Delta band saw | 88.0 dBA | Provide Protection |
| Shop | Ryobi Router | 99.3-100.1 dBA | Provide Protection |
| Shop | Skill Saw | 99.8 dBA | Provide Protection |
| Kitchen | Compressors | 72-73 dBA |  |
| Kitchen | Disposer | 78-80 dBA |  |
| Band Room | Drums and Instruments | 78-93 dBA | Provide Protection |
|  |  |  |  |

**Completed by Lee Carlson** **Date** 3-13 -2009

Note: Intend to do a general sound survey in the 2015-2016 school year to see if any changes have occurred. –EC-9/21/2015